V1.0 Release Notes

1. ZB-485-MODBUS

Channel Setup/Update works ok but it looks like ANSGCNV doesn’t store newly updated setup information to its onboard EEPROM. The net result is after ANSGCNV board reset/power recycle, all the channel setup information is lost and board is reset to its default state. This issue can only be verified only after this issue is tested with a new confirmed-working ANSGCNV board since the ANSGCNV board that was tested has been modified (hand soldered) somehow for other tests.